# pbmtonokia

Updated: 26 June 2001
Index

## NAME

pbmtonokia - convert a portable bitmap to Nokia Smart Messaging Formats

## SYNOPSIS

pbmtonokia [options] [pbmfile]

## DESCRIPTION

Reads a portable bitmap as input. Produces a Nokia Smart Messaging (hexcode, .nok, .ngg) file as output.

## OPTIONS

-fmt
  Specifies the output format (default is HEX_NOL).
HEX_NOL
  Nokia Operator Logo as (uploadable) hexcode. Use option -net to specify network code.
HEX_NGG
  Nokia Group Graphic as (uploadable) hexcode.
HEX_NMP
  Nokia Picture Message as (uploadable) hexcode. Use option -txt to specify optional text message.
NOL
  Nokia Operator Logo as .nol format. This is editable by the Group-Graphic Editor from Kessler Wireless Design (www.kessler-design.com)
NGG
  Nokia Group Graphic as .ngg format. This is editable by the Group-Graphic Editor from Kessler Wireless Design (www.kessler-design.com)
-net
  Specifies the 6 hex-digit operator network code for Operator Logos (Default is 62F210 = D1,Germany).
-txt
  Specifies the text message for Picture Messages. Default is no text message.

## LIMITATIONS

Currently limited to rows<=255 and columns<=255. Supports only b/w graphics, not animated.

## SEE ALSO

pbm, Nokia Smart Messaging Specification (http://forum.nokia.com)

## AUTHOR

Copyright (C) 2001 Tim Ruehsen <tim.ruehsen@openmediasystem.de>.

## Index

NAME
SYNOPSIS
DESCRIPTION
OPTIONS
LIMITATIONS
SEE ALSO
AUTHOR