# g3topbm

Updated: 02 October 1989
Index

## NAME

g3topbm - convert a Group 3 fax file into a portable bitmap

## SYNOPSIS

g3topbm [-kludge] [-reversebits] [-stretch] [g3file]

## DESCRIPTION

Reads a Group 3 fax file as input. Produces a portable bitmap as output.

## OPTIONS

-kludge
  Tells g3topbm to ignore the first few lines of the file; sometimes fax files have some junk at the beginning.
-reversebits
  Tells g3topbm to interpret bits least-significant first, instead of the default most-significant first. Apparently some fax modems do it one way and others do it the other way. If you get a whole bunch of "bad code word" messages, try using this flag.
-stretch
  Tells g3topbm to stretch the image vertically by duplicating each row. This is for the low-quality transmission mode.

All flags can be abbreviated to their shortest unique prefix.

## REFERENCES

The standard for Group 3 fax is defined in CCITT Recommendation T.4.

## BUGS

Probably.

## SEE ALSO

pbmtog3, pbm

## AUTHOR

Copyright (C) 1989 by Paul Haeberli <paul@manray.sgi.com>.

## Index

NAME
SYNOPSIS
DESCRIPTION
OPTIONS
REFERENCES
BUGS
SEE ALSO
AUTHOR