# yuvsplittoppm

Updated: 26 August 93
Index

## NAME

yuvplittoppm - convert a Y- and U- and a V-file into a portable pixmap.

## SYNOPSIS

yuvsplittoppm basename width height [-ccir601]

## DESCRIPTION

Reads three files, containing the YUV components, as input. These files are basename.Y, basename.U, and basename.V. Produces a portable pixmap on stdout.

Since the YUV files are raw files, the dimensions width and height must be specified on the command line.

## OPTIONS

-ccir601
  Assumes that the YUV triplets are scaled into the smaller range of the CCIR 601 (MPEG) standard. Else, the JFIF (JPEG) standard is assumed.

## SEE ALSO

ppmtoyuvsplit, yuvtoppm, ppm

## AUTHOR

Marcel Wijkstra <wijkstra@fwi.uva.nl>, based on ppmtoyuvsplit.

## Index

NAME
SYNOPSIS
DESCRIPTION
OPTIONS
SEE ALSO
AUTHOR