# ppmtolj

Updated: 4 Sept 2000
Index

## NAME

ppmtolj - convert a portable pixmap to an HP LaserJet PCL 5 Color file

## SYNOPSIS

ppmtolj [-gamma val] [-resolution 75|100|150|300|600] [-delta] [-float] [-noreset] [ppmfile]

## DESCRIPTION

Reads a portable pixmap as input and converts it into a color file suitable to be printed by an HP color PCL 5 printer.

## OPTIONS

-delta
  Apply delta row compression to reduce the size of the pcl file.
-gamma int
  Gamma correct the image using the integet parameter as a gamma (default 0).
-float
  Suppresses positioning information. The default is to write the sequence ESC&l0E to the output.
-noreset
  Prevents writing of the reset sequence to the begining and end of the output.
-resolution
  Set the required output resolution 75|100|150|300|600

## SEE ALSO

HP PCL 5 & Color Reference Guide, pnmtopclx.html, pbmtolj.html, ppmtopj, thinkjettopbm, ppm.html

## AUTHOR

Copyright (C) 2000 by Jonathan Melvin.(jonathan.melvin@heywood.co.uk)

## Index

NAME
SYNOPSIS
DESCRIPTION
OPTIONS
SEE ALSO
AUTHOR